|  | ADULT FAMILY HOME (AFH)  **AFH Initial Licensing Inspection:**  **Resident Bedroom / Bathroom Worksheet Continuation** | | Attachment E1 | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| APPLICANT’S / ER’S NAME | | | | APPLICANT CONTACT PHONE | |
| AFH NAME | | | | AFH SITE PHONE | |
| AFH SITE ADDRESS | | | DISTRICT / UNIT | | COUNTY | INSPECTION TYPE  **Initial** | | 12 MONTH DATE |
| FIELD MANAGER’S NAME | | | FM PHONE | | | LICENSOR’S NAME | | |
|  | | | | | | | | |
| **Bedroom** Measurements: Length (L) x Width (W) divided by 144 = Square Feet (Sq. Ft.) | | | | | | | | |
| Evacuation Level  I  I/ A | | Subtotal Sq. Ft. = | |  | | | | |
| - Closet / Storage | |
| - Door Swing | |
| Capacity  1  2 | | - Other | |
| - Other | |
| **= Usable Sq. Ft.** | |
| **\*M N N/A**  **Exit does not pass through another room:**  **\*M N N/A**  **Window:\*\***    Door opening device  Unobstructed    **Clean:**  Windowsill height does not exceed **Closet / Storage:**  44 inches    Open-able  Screens    Floor Guides  Privacy    **Smoke Detector:**  Open-able    Works  **Lighting:**    Audible  **Door:**    Proximity  Lock    **Heat Source:** | | | | **\*\* Window specifications: Minimum height – 24”, Minimum width – 20”, Minimum square footage opening – 5.7 sq.ft. except at grade level where it may be 5 sq.ft.** | | | | |
| **Bathroom attached to Bedroom A Water Temperature:      oF**  (Minimum 105oF; maximum 120oF)  **\*M N N/A \*M N N/A**  **Accessibility Level:** **General:**  I  I/ A    Sanitation  **Door:**    Toxics inaccessible  Lock with opening device    TP holder  Unobstructed    Toilet grab bars secure  **Shower / Tub:**    Window cover / screens  Shower / tub grab bars secure    Lighting  Non-Skid Surface    Other | | | |  | | | | |